
[basic]
version=1

[benchmark]
name=Benchmark
name[zh]=跑分测试
version=1.0.2
icon=icon.png
author=neucrack@Sipeed Ltd
desc=Hardware and software benchmark
desc[zh]=硬件和软件跑分
exec=main.py

[camera]
name=Camera
name[zh]=相机
version=1.0.0
icon=assets/camera.json
author=Sipeed Ltd
desc=Camera APP, take photos and record videos
desc[zh]=照相机应用，照相或者录制视频
exec=camera

[desktop_monitor]
name=Desktop Monitor
name[zh]=桌面监视器
version=1.0.5
icon=assets/desktop_monitor.json
author=neucrack@Sipeed Ltd
desc=Monitoring PC info, or other info from internet or local.
desc[zh]=监控电脑性能参数，或者其它来自互联网或者本地的数据。
exec=main.py

[find_blobs]
name=Find blobs
name[zh]=寻找色块
version=1.0.1
icon=assets/ball.json
author=Sipeed Ltd
desc=Find the position of the color block in camera and send the coord of the block from the communication module(Default is uart).
desc[zh]=寻找摄像头画面中的色块位置，并用通信模块(默认是uart)发送的色块的坐标
exec=find_blobs

[http_file_browser]
name=HTTP File Browser
name[zh]=HTTP 文件浏览器
version=1.1.7
author=Neucrack@Sipeed
icon=icon.json
desc=Browse and download files though http(browser)
exec=main.py

[imu_ahrs]
name=IMU AHRS
name[zh]=姿态解算
version=1.0.3
icon=assets/icon.png
author=Sipeed Ltd
desc=IMU AHRS
desc[zh]=IMU 姿态解算
exec=main.py

[line_tracking]
name=Line tracking
name[zh]=巡线
version=1.0.0
icon=assets/line_tracking.json
author=Sipeed Ltd
desc=Trace the line in camera and send the coord and theta from the communication module.
desc[zh]=巡线，用于小车机器人巡线，通过串口发送坐标和角度。
exec=line_tracking

[maixhub]
name=MaixHub Client
name[zh]=MaixHub 客户端
version=1.1.1
author=Sipeed
icon=app.png
desc=MaixHub client to collect image or deploy AI model etc.
exec=main.py

[mouse]
name=Mouse Simulator
name[zh]=鼠标模拟
version=1.0.1
author=Sipeed Ltd
icon=icon.png
desc=Simulate using a mouse to control the mouse
exec=main.py

[photos]
name=Photos
name[zh]=相册
version=1.0.1
icon=assets/photos.json
author=Sipeed Ltd
desc=Photos
desc[zh]=相册
exec=photos

[rtmp_live]
name=RTMP Live
name[zh]=RTMP 直播
version=1.0.0
icon=assets/live.json
author=Sipeed Ltd
desc=RTMP live
desc[zh]=RTMP 直播
exec=main.py

[rtsp_stream]
name=RTSP Stream
name[zh]=RTSP 推流
version=1.0.1
icon=assets/app.png
author=Sipeed Ltd
desc=RTSP stream
desc[zh]=RTSP 推流
exec=main.py

[scan_qrcode]
name=Scan QR Code
name[zh]=扫描二维码
version=1.0.0
icon=assets/scan.json
author=Sipeed Ltd
desc=Scan the qrcode/apriltag in camera screen and send the result of the qrcode from the communication module(Default is uart).
desc[zh]=扫描摄像头画面中的二维码或者Apriltag，并用通信模块(默认是uart)发送二维码的识别结果
exec=main.py

[thermal_camera]
name=Thermal Camera
name[zh]=热成像仪
version=1.0.0
icon=assets/thermal.json
author=Sipeed Ltd
desc=Thermal Camera
desc[zh]=热成像仪
exec=thermal_camera

[tof_camera]
name=ToF Camera
name[zh]=ToF
version=1.0.0
icon=assets/tof.json
author=Sipeed Ltd
desc=ToF
desc[zh]=ToF
exec=tof_camera

[uvc_camera]
name=UVC Camera
name[zh]=UVC相机
version=1.0.0
icon=assets/uvc_camera.json
author=Sipeed Ltd
desc=UVC Camera APP, show pictures on your PC
desc[zh]=UVC照相机应用，在你的电脑上显示画面
exec=uvc_camera

